# NX File Modifications Required for Drone Gimbal Arm Study

## Overview

The study uses the same beam model as `simple_beam_optimization` but requires modifications to:
1. Add modal analysis (frequency extraction)
2. Update loading conditions for the 850g camera payload
3. Ensure material properties match Al 7075-T6

## Critical Modifications

### 1. Simulation File (Beam_sim1.sim)

**REQUIRED: Add Modal Analysis Solution**

You need to add a **second solution** for modal analysis:

1. **Open** `Beam_sim1.sim` in NX Simcenter
2. **Create New Solution**:
   - Solution Type: `SOL 103 - Normal Modes`
   - Name: `modal_analysis`
   - Number of modes: `10` (we only need the first, but calculate more for safety)
   - Frequency range: `0-500 Hz`

3. **Use Same Mesh** as the static solution
   - Link to existing FEM file: `Beam_fem1.fem`

4. **Boundary Conditions**: Use same constraints as static analysis
   - Fixed constraint at base (same as static)
   - No loads needed for modal (it finds natural frequencies)

### 2. Static Analysis Modifications

**Update Load Magnitude**:

The existing static analysis load needs to represent the **850g camera payload**:

1. **Open Solution 1** (static analysis)
2. **Modify Force Magnitude**:
   - Old value: (whatever is currently there)
   - **New value**: `8.34 N` (850g × 9.81 m/s²)
   - Direction: Downward (negative Y or Z depending on your coordinate system)
   - Location: Tip of beam (where camera attaches)

Note: 120 MPa stress limit provides safety factor of 2.3 on 6061-T6 yield strength (276 MPa)

### 3. Material Properties

**Verify Material is Al 6061-T6**:

1. **Open Part File**: `Beam.prt`
2. **Check Material Assignment**:
   - Material: `Aluminum 6061-T6`
   - Yield Strength: ~276 MPa
   - Young's Modulus: ~68.9 GPa
   - Density: ~2700 kg/m³
   - Poisson's Ratio: ~0.33

3. **If not Al 6061-T6**, update material assignment to match drone application requirements

### 4. Results Configuration

**Ensure these results are requested**:

**For Static Solution (Solution 1)**:
- Displacement (VECTOR, all components)
- von Mises Stress
- Mass properties

**For Modal Solution (Solution 2)**:
- Natural frequencies
- Mode shapes (optional, for visualization)

## What You DON'T Need to Change

The parametric design variables are already set up correctly in the beam model:
- `beam_half_core_thickness` (20-30mm)
- `beam_face_thickness` (1-3mm)
- `holes_diameter` (180-280mm)
- `hole_count` (8-14)

These parameters will be automatically updated by the optimization loop.

## Verification Steps

Before running optimization, verify:

1. **Two Solutions Exist**:
   ```
   Solution 1: Static Analysis (SOL 101) - displacement and stress
   Solution 2: Modal Analysis (SOL 103) - natural frequencies
   ```

2. **Load is Correct**:
   - Static load = 8.34 N downward at tip

3. **Material is Al 7075-T6**

4. **Both solutions solve successfully** with baseline parameters:
   ```
   beam_half_core_thickness = 25mm
   beam_face_thickness = 2mm
   holes_diameter = 230mm
   hole_count = 11
   ```

## Quick Test

Run a manual solve with baseline parameters to verify:

Expected Results (approximate):
- **Mass**: ~140-150g
- **Max Displacement**: ~1-2 mm
- **Max Stress**: ~80-100 MPa
- **First Frequency**: ~120-140 Hz

If these are wildly different, check your setup.

## Extraction Configuration

The optimization engine will extract:
- **Mass**: From Solution 1 mass properties
- **Displacement**: Maximum displacement magnitude from Solution 1
- **Stress**: Maximum von Mises stress from Solution 1
- **Frequency**: First natural frequency (mode 1) from Solution 2

All extraction is automated - you just need to ensure the solutions are configured correctly.

## Optional Enhancements

If you want more realistic results:

1. **Add Gravity Load**:
   - Apply -9.81 m/s² gravity in addition to tip load
   - Represents arm's own weight during flight

2. **Add Damping** to modal analysis:
   - Structural damping ratio: ~0.02 (2%)
   - More realistic frequency response

3. **Refine Mesh** at stress concentrations:
   - Around holes
   - At base constraint
   - Better stress accuracy

But these are NOT required for the optimization to run successfully.
